Helix One Start Up

Vacuum
Wipe Down-Outside and Inside Alcohol Lint Free Towel
Clean Sensors- Plate Developer on Swab Stick
CLEAN UV LIGHT- Plate Developer and Swab Stick
Clean Heads- MONDAYS- Nozzle Restore, Press Gently do NOT wipe
Wiper Blades- Inspect and Clean with Swab Stick
Turn on INK- Turn on INK
Check Coolent
Turn On Air FILTER- Check Filter Every Friday
Turn on Helix One Printer
Turn on HMI once Helix is in Home Screen on Key Pad
Select Part on Helix Key Pad(2=CC, 4=Tumbler)
HOME Chucks
Turn on Ripper- Rip Artwork, Select Part, Open in Editor 
Ripper Editor- Select-Color Correct- SPOT COLORS 1-2-3
Ripper Editor- Select-Print and rename ripped artwork
ABREV Name CCorT V- FFN date-attempts
Open HMI File- Select Coating Box
Check- Part, Artwork, Spot Color Press DOWNLOAD
Put Part in Chuck
Go To Load-On Helix Key
Purge INK 3 times on Monday, once every start up
AUTO CLEAN
Print, Confirm Print
GREEN Button